## Setting Up the MAX+PLUS II/Cadence Concept Work Environment for a Sun SPARCstation Running SunOS Software

If you are using Concept software on a Sun SPARCstation running SunOS software, you should also install the redifnet EDIF netlist reader utility to convert Concept schematics into MAX+PLUS II-compatible EDIF netlist files. To install the redifnet utility, follow these steps:

1. Copy the redifnet directory from the /usr/maxplus2/simlib/concept/edifnet directory to the Cadence system directory.

2. Copy the redifnet and pinmap_start files from the /usr/maxplus2/simlib/concept/edifnet/bin directory to the /<Cadence system directory path>/tools/bin.

3. Specify the -/usr/maxplus2/simlib/concept/edifnet/max2sim map file as a `PIN_MAP_FILE` in the redifnet.cmd file.

4. (Optional) Modify existing templates for directive files such as compiler.cmd, vloglink.cmd, and global.cmd. These templates are located in the /usr/maxplus2/simlib/concept/edifnet/templates directory.

5. (Optional) Modify the expansion.dat and max2sim.map files in the /usr/maxplus2/simlib/concept/edifnet directory.

Last Updated: August 28, 2000 for MAX+PLUS II version 10.0 |
| Home | List by Vendor | List by Tool | List by Function | Cadence Topics | Concept Topics | Documentation Conventions Copyright © 2000 Altera Corporation, 101 Innovation Drive, San Jose, California 95134, USA. All rights reserved. By accessing any information on this CD-ROM, you agree to be bound by the terms of Altera's Legal Notice.