## MAX+PLUS II Project File Structure

In MAX+PLUS® II, a project name is the name of a top-level design file, without the filename extension. This design file can be an EDIF, Verilog HDL, or VHDL netlist file; an AHDL™ TDF; or any other MAX+PLUS II-supported design file. The EDIF netlist file must be created by Synopsys and imported into MAX+PLUS II as an EDIF Input File.

MAX+PLUS II stores the connectivity data on the links between design files in a hierarchical project in a Hierarchy Interconnect File (.hif), but refers to the entire project only by its project name. The MAX+PLUS II Compiler uses the HIF to build a single, fully flattened project database that integrates all the design files in a project hierarchy.

Last Updated: August 28, 2000 for MAX+PLUS II version 10.0 |
| Home | List by Vendor | List by Tool | List by Function| Documentation Conventions Copyright © 2000 Altera Corporation, 101 Innovation Drive, San Jose, California 95134, USA. All rights reserved. By accessing any information on this CD-ROM, you agree to be bound by the terms of Altera's Legal Notice.