## MAX+PLUS II/Cadence Interface File Organization

Table 1 shows the MAX+PLUS® II/Cadence interface subdirectories that are created in the MAX+PLUS II system directory (by default, the /usr/maxplus2 directory) during MAX+PLUS II installation. For information on the other directories that are created during MAX+PLUS II installation, see "MAX+PLUS II File Organization" in MAX+PLUS II Installation in the MAX+PLUS II Getting Started manual.

#### Table 1. MAX+PLUS II Directory Organization

Directory | Description
./lmf | Contains the Altera-provided Library Mapping File, cadence.lmf, that maps Cadence logic functions to equivalent MAX+PLUS II logic functions.
./examples/cadence | Contains the sample files for Cadence software discussed in these ACCESSSM Key Guidelines.
./cadence | Contains the AMPLE userware for the MAX+PLUS II/Cadence interface.
./simlib/concept/alt_max2 | Contains the MAX+PLUS II primitives, including `CARRY`, `CASCADE`, `EXP`, `GLOBAL`, `LCELL`, `SOFT`, `OPNDRN`, `DFFE` (D flipflop with Clock Enable), and `DFFE6K` (D flipflop with Clock Enable and both Clear and Preset for FLEX® 6000 devices only) for use with Concept software.
./simlib/composer/alt_max2 | Contains the MAX+PLUS II primitives, including `CARRY`, `CASCADE`, `EXP`, `GLOBAL`, `LCELL`, `SOFT`, `OPNDRN`, `DFFE` (D flipflop with Clock Enable), and `DFFE6K` (D flipflop with Clock Enable and both Clear and Preset for FLEX 6000 devices only) for use with Composer software.
./simlib/concept/alt_lpm | Contains the MAX+PLUS II megafunctions, including library of parameterized modules (LPM) functions, for use with Concept software.
./simlib/concept/max2sim | Contains the MAX+PLUS II/Concept simulation model library, max2_sim, for use with RapidSIM software.
./simlib/concept/alt_syn | Contains the MAX+PLUS II synthesis library, alt_syn, for use with Synergy and Concept software, and the vlog2alt utility.
./simlib/composer/alt_syn | Contains the MAX+PLUS II synthesis library, alt_syn, for use with Synergy and Composer software.
./simlib/concept/lpm_syn | Contains the Cadence LPM library, lpm_syn, for use with Synergy and Concept software.
./simlib/composer/lpm_syn | Contains the Cadence LPM library, lpm_syn, for use with Synergy and Composer software.
./simlib/concept/alt_mf | Contains the MAX+PLUS II VHDL logic function library. (`a_8count` is for the MAX® 7000 and MAX 9000 device families only.)
./simlib/concept/edifnet/templates | Contains template files for Concept directives, i.e., global.cmd, compiler.cmd, vloglink.cmd, verilog.cmd, and master.local.
./simlib/concept/alt_max2/verilogUdps | Contains Verilog HDL modules that are the equivalent of the primitives contained in alt_max2 library for use with Concept software.
./simlib/composer/alt_max2/verilogUdps | Contains Verilog HDL modules that are the equivalent of the primitives contained in alt_max2 library for use with Composer software.
./simlib/concept/alt_vtl ./simlib/composer/alt_vtl | Contains VITAL library source files for use with Concept or Composer software.
./simlib/composer/alt_max2/verilog | Contains simulation modules for all symbols in the alt_max2 Composer library.

| Go to the following topics, which are available on the web, for additional information:

- MAX+PLUS II Getting Started version 8.1 (5.4 MB)
- This manual is also available in 4 parts:
  - Preface & Section 1: MAX+PLUS II Installation
  - Section 2: MAX+PLUS II - A Perspective
  - Section 3: MAX+PLUS II Tutorial
  - Appendices, Glossary & Index
- FLEX Devices
- MAX Devices
- Classic Device Family

Last Updated: August 28, 2000 for MAX+PLUS II version 10.0 |
| Home | List by Vendor | List by Tool | List by Function | Cadence Topics | Documentation Conventions Copyright © 1995-2000 Altera Corporation, 101 Innovation Drive, San Jose, California 95134, USA. All rights reserved. By accessing any information on this CD-ROM, you agree to be bound by the terms of Altera's Legal Notice.