## Compiling the alt_mf Library

If your VHDL design uses functions from the alt_mf library, you must compile this library. To compile the alt_mf library, follow these steps:

1. Be sure to set up your working environment correctly, as described in Setting Up the MAX+PLUS® II/Cadence Working Environment. For example, you must ensure that the appropriate directories are specified in the cds.lib file located in your working directory.

2. Change to the alt_mf directory by typing `cd /usr/maxplus2/simlib/concept/alt_mf` at the UNIX prompt.

3. Edit the hdl.var file located in your working directory to include the following line:

   `DEFINE work alt_mf`

4. Type the following commands at the UNIX prompt from the /usr/maxplus2/simlib/concept/alt_mf directory to compile the library:

   `cv -message -file ./src/mf.vhd`
   `cv -message -file ./src/mf_components.vhd`

Last Updated: August 28, 2000 for MAX+PLUS II version 10.0 |
| Home | List by Vendor | List by Tool | List by Function | Cadence Topics | Leapfrog Topics | Documentation Conventions Copyright © 2000 Altera Corporation, 101 Innovation Drive, San Jose, California 95134, USA. All rights reserved. By accessing any information on this CD-ROM, you agree to be bound by the terms of Altera's Legal Notice.